**DRY MOLY**

**“NEW & IMPROVED”**

**AEROSOL DRY LUBRICANT**

**PRODUCT**

INFORMATION**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**DESCRIPTION Dry Moly** is a superior dry film lubricant, formulated with molybdenum for long

 lasting lubrication and anti-seize properties. **Dry Moly** withstands high pressure,

 high temperatures, water and chemical attack. The dry film is ideal for use in

 dusty, dirty locations by avoiding dirty build-ups. **Dry Moly** provides excellent

 lubrication properties without attraction of dust or dirt creating a smooth,

 frictionless surface for maximum operating efficiency.

**USE Dry Moly** reduces metal wear and fatigue to extend equipment life and will not

 break down under high temperatures. Use **Dry Moly** on gears, chains, motors,

 bearings, boilers, engines, pump assemblies, conveyors, construction equipment,

 farm implement equipment.

**DIRECTIONS** Shake well before use. Spray 8-10 inches from surface. Spray a light even

Film. Wipe off excess with cloth and repeat application. A second coat gives

 Additional protection.

**WARNING** Keep away from heat, sparks, or open flame. Effects of overexposure include

irritation of respiratory tract, headache, dizziness, nausea, and loss of coordination. Always read label before using product.

**KEEP OUT OF REACH OF CHILDREN.**

**FIRST AID** SKIN: Immediately flush exposed area with water for at least 15 minutes.

 If irritation persists, get medical attention. Remove contaminated clothing

 and launder before reuse.

 EYES: Immediately flush with large quantities of water for at least 15 minutes,

 lifting upper and lower eyelids occasionally. Seek medical attention.

 INHALATION: Remove person to fresh air. If irritation persists, give oxygen.

 Get medical attention.

 INGESTION: DO NOT induce vomiting. Seek medical attention immediately.

 Note: Never give anything by mouth to an unconscious or convulsing victim.

 Keep person warm and quiet.

1365 Revised 092413

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_­­­\_\_\_\_\_\_\_\_**

CORRELATED

 Chemistry

CORRELATED PRODUCTS, INC

5616 PROGRESS ROAD / PO BOX 42387 / INDIANAPOLIS IN 46242-0387

PHONE 317/243-3248 / FAX 317/244/8461 / TOLL FREE 1/800/428-3266