

**Molycor System**

**General Application Information**

**Single-axle dump truck with moderate rust, treating the underbody only**

½ Gallon Molycor Plus

½ Gallon Arrest

1 Quart Clion

**Double-axle dump truck with moderate rust, treating the underbody only:**

¾ Gallon Molycor Plus

1 Gallon Arrest

2 Quart Clion

**To include the dump body for the single-axle truck, add:**

½ Gallon Molycor Plus

½ Gallon Arrest

1 Quart Clion

**To include the dump body for the double-axle truck, add:**

1 Gallon Molycor Plus

1 Gallon Arrest

2 Quarts Clion X

Treatment quantities vary depending on the size of the truck and the amount of rust being treated or removed.

Invite our regional manager in to show you how easy it is to use these products.

   

 CLION-X SALT & CHLORIDE WASH ARREST-RUST REMOVAL/ MOLYCOR UNDERCOAT

 COVERSION

5616 Progress Road

Indianapolis, IN 46241

317-243-3248\*800-428-3266

[www.CPIRoadSolutions.com](http://cpiroadsolutions.com/product-category/cpi/cpi-automotive-fleet-maintenance/molycor-system/)